{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Feuille1","Feuille2","Feuille3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Feuille1","index":0,"n_rows":44,"n_cols":3,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["FICHE AVION","C150"]
[]
["Envergure","10,11 m"]
["Masse max","726 kg"]
["Masse vide","515 kg"]
["Charge utile","152 kg"]
[]
["Moteur"]
["Qte Huile","6 quarts"]
["Type essence ","80/87 100L"]
["Qte essence","85 l (59,5kg)"]
["Autonomie ","4 h"]
["Conso 2500ft 2600tr/min","20,4 l"]
[]
["Distance Piste dur MSL"]
["Décollage","422 m"]
["Roulage","224 m"]
["Atterrissage","328 m"]
["Roulage","136 m"]
[]
["Limitation vents travers"]
["Décollage","20 kts"]
["Atterrissage","15 kts"]
[]
["Vitesse"]
[]
["VNE","141 kts"]
["VNO","104 kts"]
["VA","95 kts"]
["VFE","87 kts"]
["V finesse max","61 kts"]
["V rotation","48 kts"]
["Vy","68 kts"]
["Vx (sans volet)","61 kts"]
["V croisiere 2525 Tr/min","100 kts"]
["V descente volet 10°","65 kts"]
["V descente volet 20°","60 kts"]
["V descente volet 40°","55 kts"]
[]
["Decrochage"]
["Volet","vitesse","Marge 30 %"]
["0°","48 kts","63 kts"]
["20°","43 kts","56 kts"]
["40°","42 kts","55 kts"]

{"sheet":"Feuille2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Feuille3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}