{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Feuil1","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Feuil1","index":0,"n_rows":36,"n_cols":5,"rows_kept":36,"cut":false,"hidden":false,"merged":[[30,0,32,0],[33,0,35,0],[0,0,2,4],[4,0,7,0],[8,0,11,0],[12,0,15,0],[16,0,20,0],[21,0,23,0],[24,0,26,0],[27,0,29,0]],"flags":["formulas_cached_only"]}
["COMMUTATEURS ROTATIF ET INTERRUPTEURS 3 POSITIONS"]
[]
[]
["FONCTIONS FALCON 4 AF","POSITION","CLAVIER","LOIOCP","ENTREE IOCARD"]
["AIR SOURCE","OFF","S à",32779]
[null,"NORM","C à",523]
[null,"DUMP","A à",267]
[null,"RAM","SC à",33291]
["INS","OFF","SCA &",33538]
[null,"NORM","SCA é",33539]
[null,"NAV","SCA \"",33540]
[null,"IN FLIGHT","SCA '",33541]
["EWS PROGRAMME","PGM 1","SCA e",33554]
[null,"PGM 2","SCA r",33555]
[null,"PGM 3","SCA t",33556]
[null,"PGM 4","SCA y",33557]
["EWS MODE","OFF","SCA u",33558]
[null,"STANDBY","SCA i",33559]
[null,"MANUEL","SCA o",33560]
[null,"SEMI","SCA *",33579]
[null,"AUTO","SCA ù",33576]
["LEFT AP SWITCH","UP","SC &",33282]
[null,"MIDDLE","C &",514]
[null,"DOWN","SCA l",33574]
["RIGHT AP SWITCH","UP","SC é",33283]
[null,"MIDLE","C é",515]
[null,"DOWN","SCA n",33585]
["MAIN POWER","OFF","CA F1",827]
[null,"BATT","CA F2",828]
[null,"MAIN","S F1",32827]
["SPEED","GND","SC !",33333]
[null,"CAS","SC :",33332]
[null,"TAS","SC ;",33331]
["ALTITUDE","RADAR","SA !",33077]
[null,"BARO","SA ;",33075]
[null,"AUTO","SA ,",33074]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}